
**Date Submitted: 11/10/18 4:20 PM**


**Task 01:**

Youtube Link: <https://www.youtube.com/watch?v=dBxoWVG_qa0>


The output ROV readings of the Clock Module in the empty.cfg file:




Here is the output within the Live Session tab with a filter to search for the keyword “LED”. This is seen when going on the execution analysis setting.



Below is the Execution Graph, between the 2 markers shows about 307 cycles.



Below is the instance for Clock called “ledToggleClk” where we will call the function ledToggle.



Modified Code:

//---------------------------------------------------------------------------------

// Project: Blink TM4C BIOS Using Clock Fxns (STARTER)

// Author: Eric Wilbur

// Date: June 2014

//

// Note: The function call TimerIntClear(TIMER2\_BASE, TIMER\_TIMA\_TIMEOUT) HAS

// to be in the ISR. This fxn clears the TIMER's interrupt flag coming

// from the peripheral - it does NOT clear the CPU interrupt flag - that

// is done by hardware. The author struggled figuring this part out - hence

// the note. And, in the Swi lab, this fxn must be placed in the

// Timer\_ISR fxn because it will be the new ISR.

//

// Follow these steps to create this project in CCSv6.0:

// 1. Project -> New CCS Project

// 2. Select Template:

// - TI-RTOS for Tiva-C -> Driver Examples -> EK-TM4C123 LP -> Example Projects ->

// Empty Project

// - Empty Project contains full instrumentation (UIA, RTOS Analyzer) and

// paths set up for the TI-RTOS version of MSP430Ware

// 3. Delete the following files:

// - Board.h, empty.c, EK\_TM4C123GXL.c/h, empty\_readme.txt

// 4. Add main.c from TI-RTOS Workshop Solution file for this lab

// 5. Edit empty.cfg as needed (to add/subtract) BIOS services, delete given Task

// 6. Build, load, run...

//----------------------------------------------------------------------------------

//----------------------------------------

// BIOS header files

//----------------------------------------

**#include** <xdc/std.h> //mandatory - have to include first, for BIOS types

**#include** <ti/sysbios/BIOS.h> //mandatory - if you call APIs like BIOS\_start()

**#include** <xdc/runtime/Log.h> //needed for any Log\_info() call

**#include** <xdc/cfg/global.h> //header file for statically defined objects/handles

**#include** <xdc/runtime/Timestamp.h> // used for Timestamp() calls

//------------------------------------------

// TivaWare Header Files

//------------------------------------------

**#include** <stdint.h>

**#include** <stdbool.h>

**#include** "inc/hw\_types.h"

**#include** "inc/hw\_memmap.h"

**#include** "driverlib/sysctl.h"

**#include** "driverlib/gpio.h"

**#include** "inc/hw\_ints.h"

**#include** "driverlib/interrupt.h"

**#include** "driverlib/timer.h"

//----------------------------------------

// Prototypes

//----------------------------------------

**void** **hardware\_init**(**void**);

**void** **ledToggle**(**void**);

//void Timer\_ISR(void);

//---------------------------------------

// Globals

//---------------------------------------

**volatile** int16\_t i16ToggleCount = 0;

//---------------------------------------------------------------------------

// main()

//---------------------------------------------------------------------------

**void** **main**(**void**)

{

hardware\_init(); // init hardware via Xware

BIOS\_start();

}

//---------------------------------------------------------------------------

// hardware\_init()

//

// inits GPIO pins for toggling the LED

//---------------------------------------------------------------------------

**void** **hardware\_init**(**void**)

{

uint32\_t ui32Period;

//Set CPU Clock to 40MHz. 400MHz PLL/2 = 200 DIV 5 = 40MHz

**SysCtlClockSet**(SYSCTL\_SYSDIV\_5|SYSCTL\_USE\_PLL|SYSCTL\_XTAL\_16MHZ|SYSCTL\_OSC\_MAIN);

// ADD Tiva-C GPIO setup - enables port, sets pins 1-3 (RGB) pins for output

**SysCtlPeripheralEnable**(SYSCTL\_PERIPH\_GPIOF);

**GPIOPinTypeGPIOOutput**(GPIO\_PORTF\_BASE, GPIO\_PIN\_1|GPIO\_PIN\_2|GPIO\_PIN\_3);

// Turn on the LED

**GPIOPinWrite**(GPIO\_PORTF\_BASE, GPIO\_PIN\_1|GPIO\_PIN\_2|GPIO\_PIN\_3, 4);

/\*

// Timer 2 setup code

SysCtlPeripheralEnable(SYSCTL\_PERIPH\_TIMER2); // enable Timer 2 periph clks

TimerConfigure(TIMER2\_BASE, TIMER\_CFG\_PERIODIC); // cfg Timer 2 mode - periodic

ui32Period = (SysCtlClockGet() /2); // period = CPU clk div 2 (500ms)

TimerLoadSet(TIMER2\_BASE, TIMER\_A, ui32Period); // set Timer 2 period

TimerIntEnable(TIMER2\_BASE, TIMER\_TIMA\_TIMEOUT); // enables Timer 2 to interrupt CPU

TimerEnable(TIMER2\_BASE, TIMER\_A); // enable Timer 2

\*/

}

//---------------------------------------------------------------------------

// ledToggle()

//

// toggles LED on Tiva-C LaunchPad

//---------------------------------------------------------------------------

**void** **ledToggle**(**void**)

{

**static** uint32\_t ui32\_t0, ui32\_t1, ui32\_t2, ui32start, ui32stop, ui32delta; // used for Timestamp calculations

ui32\_t0 = Timestamp\_get32(); // calculate Timestamp() overhead (ui32\_t2)

ui32\_t1 = Timestamp\_get32();

ui32\_t2 = ui32\_t1 - ui32\_t0;

// LED values - 2=RED, 4=BLUE, 8=GREEN

**if**(**GPIOPinRead**(GPIO\_PORTF\_BASE, GPIO\_PIN\_2))

{

ui32start = Timestamp\_get32(); // get starting Timer snapshot for LED benchmark

**GPIOPinWrite**(GPIO\_PORTF\_BASE, GPIO\_PIN\_1|GPIO\_PIN\_2|GPIO\_PIN\_3, 0); // toggle GPIO/LED

ui32stop = Timestamp\_get32(); // get ending Timer snapshot for LED benchmark

ui32delta = ui32stop - ui32start - ui32\_t2; // calculate LED toggle benchmark

Log\_info1("LED BENCHMARK = [%u] TM4C CYCLES", ui32delta); // send LED benchmark to Log display

}

**else**

{

**GPIOPinWrite**(GPIO\_PORTF\_BASE, GPIO\_PIN\_2, 4);

}

i16ToggleCount += 1; // keep track of #toggles

Log\_info1("LED TOGGLED [%u] TIMES",i16ToggleCount); // send toggle count to UIA

}

//---------------------------------------------------------------------------

// Timer ISR - called by BIOS Hwi (see app.cfg)

//

// Posts Swi (or later a Semaphore) to toggle the LED

//---------------------------------------------------------------------------

/\*void Timer\_ISR(void)

{

TimerIntClear(TIMER2\_BASE, TIMER\_TIMA\_TIMEOUT); // must clear timer flag FROM timer

Swi\_post(LEDSwi); // post LEDSwi

}\*/